;mcr_Group##OTHER##;mcr_Family##OTHER##;mcr_Nominal dimensions (roof opening dim.)##OTHER##;mcr_Nominal width##LENGTH##MILLIMETERS;mcr_Nominal length##LENGTH##MILLIMETERS;mcr_Active area##AREA##SQUARE_METERS;mcr_Active area with wind deflectors##AREA##SQUARE_METERS;mcr_Active area with wind deflectors and inlet deflector##AREA##SQUARE_METERS;mcr_Pneumatic control - parameters##OTHER##;mcr_Weight##MASS##KILOGRAMS;mcr_Base type##OTHER##;mcr_Notes##OTHER##;URL##OTHER##;Type Comments##OTHER##;Model##OTHER##;Manufacturer##OTHER##;Description##OTHER##;mcr_Code##OTHER##;mcr_Smoke vent with roof access function##OTHER##;mcr_c_b1##LENGTH##MILLIMETERS;mcr_c_h1##LENGTH##MILLIMETERS;mcr_How##LENGTH##MILLIMETERS
E 80x120;Smoke vent;mcr ULTRA THERM;80x120 cm;800;1200;0.38;0;0;Pneumatic control SL750;70;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 80x120;Mercor S.A.;Smoke vent mcr ULTRA THERM;8001200;0;175;275;154
E 90x120;Smoke vent;mcr ULTRA THERM;90x120 cm;900;1200;0.43;0;0;Pneumatic control SL750;75;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 90x120;Mercor S.A.;Smoke vent mcr ULTRA THERM;9001200;0;175;275;154
C 100;Smoke vent;mcr ULTRA THERM;100x100 cm;1000;1000;0.72;0.71;0.79;Pneumatic control SL750;70;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM C 100;Mercor S.A.;Smoke vent mcr ULTRA THERM;10001000;0;175;297;214
E 100x110;Smoke vent;mcr ULTRA THERM;100x110 cm;1000;1100;0.79;0.78;0.87;Pneumatic control SL750;75;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 100x110;Mercor S.A.;Smoke vent mcr ULTRA THERM;10001100;0;175;297;194
E 100x120;Smoke vent;mcr ULTRA THERM;100x120 cm;1000;1200;0.85;0.84;0.95;Pneumatic control SL750;75;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 100x120;Mercor S.A.;Smoke vent mcr ULTRA THERM;10001200;0;175;297;174
E 100x130;Smoke vent;mcr ULTRA THERM;100x130 cm;1000;1300;0.92;0.91;1.03;Pneumatic control SL750;80;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 100x130;Mercor S.A.;Smoke vent mcr ULTRA THERM;10001300;0;175;297;174
E 100x140;Smoke vent;mcr ULTRA THERM;100x140 cm;1000;1400;0.98;0.98;1.11;Pneumatic control SL750;80;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 100x140;Mercor S.A.;Smoke vent mcr ULTRA THERM;10001400;0;175;297;154
E 100x150;Smoke vent;mcr ULTRA THERM;100x150 cm;1000;1500;1.04;1.05;1.19;Pneumatic control SL750;85;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 100x150;Mercor S.A.;Smoke vent mcr ULTRA THERM;10001500;0;175;297;154
E 100x160;Smoke vent;mcr ULTRA THERM;100x160 cm;1000;1600;1.1;1.12;1.26;Pneumatic control SL750;90;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 100x160;Mercor S.A.;Smoke vent mcr ULTRA THERM;10001600;0;175;297;174
E 100x170;Smoke vent;mcr ULTRA THERM;100x170 cm;1000;1700;1.16;1.18;1.35;Pneumatic control SL750;90;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 100x170;Mercor S.A.;Smoke vent mcr ULTRA THERM;10001700;0;175;297;194
E 100x180;Smoke vent;mcr ULTRA THERM;100x180 cm;1000;1800;1.22;1.24;1.44;Pneumatic control SL750;95;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 100x180;Mercor S.A.;Smoke vent mcr ULTRA THERM;10001800;0;175;297;194
E 100x190;Smoke vent;mcr ULTRA THERM;100x190 cm;1000;1900;1.28;1.31;1.52;Pneumatic control SL750;95;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 100x190;Mercor S.A.;Smoke vent mcr ULTRA THERM;10001900;0;175;297;194
E 100x200;Smoke vent;mcr ULTRA THERM;100x200 cm;1000;2000;1.34;1.38;1.6;Pneumatic control SL750;100;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 100x200;Mercor S.A.;Smoke vent mcr ULTRA THERM;10002000;0;175;297;214
E 100x210;Smoke vent;mcr ULTRA THERM;100x210 cm;1000;2100;1.4;1.45;1.68;Pneumatic control SL750;100;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 100x210;Mercor S.A.;Smoke vent mcr ULTRA THERM;10002100;0;175;297;214
E 100x220;Smoke vent;mcr ULTRA THERM;100x220 cm;1000;2200;1.45;1.52;1.76;Pneumatic control SL750;105;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 100x220;Mercor S.A.;Smoke vent mcr ULTRA THERM;10002200;0;175;297;214
E 100x230;Smoke vent;mcr ULTRA THERM;100x230 cm;1000;2300;1.51;1.59;1.84;Pneumatic control SL750;105;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 100x230;Mercor S.A.;Smoke vent mcr ULTRA THERM;10002300;0;175;297;214
E 100x240;Smoke vent;mcr ULTRA THERM;100x240 cm;1000;2400;1.56;1.66;1.92;Pneumatic control SL750;110;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 100x240;Mercor S.A.;Smoke vent mcr ULTRA THERM;10002400;0;175;297;234
E 100x250;Smoke vent;mcr ULTRA THERM;100x250 cm;1000;2500;1.61;1.73;2;Pneumatic control SL750;110;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 100x250;Mercor S.A.;Smoke vent mcr ULTRA THERM;10002500;0;175;297;234
C 110;Smoke vent;mcr ULTRA THERM;110x110 cm;1100;1100;0.85;0.85;0.96;Pneumatic control SL750;80;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM C 110;Mercor S.A.;Smoke vent mcr ULTRA THERM;11001100;0;175;297;214
E 110x120;Smoke vent;mcr ULTRA THERM;110x120 cm;1100;1200;0.92;0.92;1.05;Pneumatic control SL750;80;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 110x120;Mercor S.A.;Smoke vent mcr ULTRA THERM;11001200;0;175;297;194
E 110x130;Smoke vent;mcr ULTRA THERM;110x130 cm;1100;1300;0.99;1;1.13;Pneumatic control SL750;85;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 110x130;Mercor S.A.;Smoke vent mcr ULTRA THERM;11001300;0;175;297;174
E 110x140;Smoke vent;mcr ULTRA THERM;110x140 cm;1100;1400;1.06;1.07;1.22;Pneumatic control SL750;85;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 110x140;Mercor S.A.;Smoke vent mcr ULTRA THERM;11001400;0;175;297;174
E 110x150;Smoke vent;mcr ULTRA THERM;110x150 cm;1100;1500;1.13;1.15;1.31;Pneumatic control SL750;90;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 110x150;Mercor S.A.;Smoke vent mcr ULTRA THERM;11001500;0;175;297;154
E 110x160;Smoke vent;mcr ULTRA THERM;110x160 cm;1100;1600;1.19;1.22;1.4;Pneumatic control SL750;90;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 110x160;Mercor S.A.;Smoke vent mcr ULTRA THERM;11001600;0;175;297;154
E 110x170;Smoke vent;mcr ULTRA THERM;110x170 cm;1100;1700;1.26;1.29;1.49;Pneumatic control SL750;95;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 110x170;Mercor S.A.;Smoke vent mcr ULTRA THERM;11001700;0;175;297;254
E 110x180;Smoke vent;mcr ULTRA THERM;110x180 cm;1100;1800;1.32;1.37;1.58;Pneumatic control SL750;95;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 110x180;Mercor S.A.;Smoke vent mcr ULTRA THERM;11001800;0;175;297;254
E 110x190;Smoke vent;mcr ULTRA THERM;110x190 cm;1100;1900;1.39;1.44;1.67;Pneumatic control SL750;100;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 110x190;Mercor S.A.;Smoke vent mcr ULTRA THERM;11001900;0;175;297;254
E 110x200;Smoke vent;mcr ULTRA THERM;110x200 cm;1100;2000;1.45;1.52;1.76;Pneumatic control SL750;100;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 110x200;Mercor S.A.;Smoke vent mcr ULTRA THERM;11002000;0;175;297;274
E 110x210;Smoke vent;mcr ULTRA THERM;110x210 cm;1100;2100;1.51;1.59;1.85;Pneumatic control SL750;105;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 110x210;Mercor S.A.;Smoke vent mcr ULTRA THERM;11002100;0;175;297;274
E 110x220;Smoke vent;mcr ULTRA THERM;110x220 cm;1100;2200;1.57;1.66;1.94;Pneumatic control SL750;105;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 110x220;Mercor S.A.;Smoke vent mcr ULTRA THERM;11002200;0;175;297;274
E 110x230;Smoke vent;mcr ULTRA THERM;110x230 cm;1100;2300;1.63;1.74;2.03;Pneumatic control SL750;110;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 110x230;Mercor S.A.;Smoke vent mcr ULTRA THERM;11002300;0;175;297;274
E 110x240;Smoke vent;mcr ULTRA THERM;110x240 cm;1100;2400;1.69;1.81;2.12;Pneumatic control SL550;110;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL550  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 110x240;Mercor S.A.;Smoke vent mcr ULTRA THERM;11002400;0;240;432;294
E 110x250;Smoke vent;mcr ULTRA THERM;110x250 cm;1100;2500;1.75;1.88;2.21;Pneumatic control SL750;115;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 110x250;Mercor S.A.;Smoke vent mcr ULTRA THERM;11002500;0;240;432;294
C 115;Smoke vent;mcr ULTRA THERM;115x115 cm;1150;1150;0.91;0.93;1.04;Pneumatic control SL550;80;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL550  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM C 115;Mercor S.A.;Smoke vent mcr ULTRA THERM;11501150;0;240;432;214
C 120;Smoke vent;mcr ULTRA THERM;120x120 cm;1200;1200;0.98;1.01;1.14;Pneumatic control SL750;85;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM C 120;Mercor S.A.;Smoke vent mcr ULTRA THERM;12001200;0;175;284;214
E 120x130;Smoke vent;mcr ULTRA THERM;120x130 cm;1200;1300;1.06;1.08;1.24;Pneumatic control SL750;85;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 120x130;Mercor S.A.;Smoke vent mcr ULTRA THERM;12001300;0;175;284;194
E 120x140;Smoke vent;mcr ULTRA THERM;120x140 cm;1200;1400;1.13;1.16;1.34;Pneumatic control SL750;90;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 120x140;Mercor S.A.;Smoke vent mcr ULTRA THERM;12001400;0;175;284;194
E 120x150;Smoke vent;mcr ULTRA THERM;120x150 cm;1200;1500;1.21;1.24;1.44;Pneumatic control SL750;90;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 120x150;Mercor S.A.;Smoke vent mcr ULTRA THERM;12001500;0;175;284;174
E 120x160;Smoke vent;mcr ULTRA THERM;120x160 cm;1200;1600;1.28;1.33;1.53;Pneumatic control SL750;95;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 120x160;Mercor S.A.;Smoke vent mcr ULTRA THERM;12001600;0;175;284;154
E 120x170;Smoke vent;mcr ULTRA THERM;120x170 cm;1200;1700;1.35;1.41;1.63;Pneumatic control SL750;95;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 120x170;Mercor S.A.;Smoke vent mcr ULTRA THERM;12001700;0;175;284;154
E 120x180;Smoke vent;mcr ULTRA THERM;120x180 cm;1200;1800;1.42;1.49;1.73;Pneumatic control SL750;100;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 120x180;Mercor S.A.;Smoke vent mcr ULTRA THERM;12001800;0;175;284;154
E 120x190;Smoke vent;mcr ULTRA THERM;120x190 cm;1200;1900;1.49;1.57;1.82;Pneumatic control SL750;105;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 120x190;Mercor S.A.;Smoke vent mcr ULTRA THERM;12001900;0;175;284;314
E 120x200;Smoke vent;mcr ULTRA THERM;120x200 cm;1200;2000;1.56;1.66;1.92;Pneumatic control SL750;105;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 120x200;Mercor S.A.;Smoke vent mcr ULTRA THERM;12002000;0;175;284;314
E 120x210;Smoke vent;mcr ULTRA THERM;120x210 cm;1200;2100;1.62;1.71;2.02;Pneumatic control SL750;110;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 120x210;Mercor S.A.;Smoke vent mcr ULTRA THERM;12002100;0;175;465;314
E 120x220;Smoke vent;mcr ULTRA THERM;120x220 cm;1200;2200;1.69;1.8;2.11;Pneumatic control SL750;110;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 120x220;Mercor S.A.;Smoke vent mcr ULTRA THERM;12002200;0;175;465;314
E 120x230;Smoke vent;mcr ULTRA THERM;120x230 cm;1200;2300;1.76;1.89;2.21;Pneumatic control SL750;115;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 120x230;Mercor S.A.;Smoke vent mcr ULTRA THERM;12002300;0;175;465;314
E 120x240;Smoke vent;mcr ULTRA THERM;120x240 cm;1200;2400;1.82;1.96;2.3;Pneumatic control SL750;115;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 120x240;Mercor S.A.;Smoke vent mcr ULTRA THERM;12002400;0;175;465;314
E 120x250;Smoke vent;mcr ULTRA THERM;120x250 cm;1200;2500;1.88;2.04;2.4;Pneumatic control SL750;120;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 120x250;Mercor S.A.;Smoke vent mcr ULTRA THERM;12002500;0;175;284;314
C 130;Smoke vent;mcr ULTRA THERM;130x130 cm;1300;1300;1.13;1.17;1.35;Pneumatic control SL750;95;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM C 130;Mercor S.A.;Smoke vent mcr ULTRA THERM;13001300;0;250;560;214
E 130x140;Smoke vent;mcr ULTRA THERM;130x140 cm;1300;1400;1.21;1.26;1.45;Pneumatic control SL750;95;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 130x140;Mercor S.A.;Smoke vent mcr ULTRA THERM;13001400;0;250;560;194
E 130x150;Smoke vent;mcr ULTRA THERM;130x150 cm;1300;1500;1.28;1.35;1.56;Pneumatic control SL750;100;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 130x150;Mercor S.A.;Smoke vent mcr ULTRA THERM;13001500;0;250;560;194
E 130x160;Smoke vent;mcr ULTRA THERM;130x160 cm;1300;1600;1.36;1.44;1.66;Pneumatic control SL750;105;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 130x160;Mercor S.A.;Smoke vent mcr ULTRA THERM;13001600;0;250;560;174
E 130x170;Smoke vent;mcr ULTRA THERM;130x170 cm;1300;1700;1.44;1.52;1.77;Pneumatic control SL750;105;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 130x170;Mercor S.A.;Smoke vent mcr ULTRA THERM;13001700;0;250;560;174
E 130x180;Smoke vent;mcr ULTRA THERM;130x180 cm;1300;1800;1.51;1.61;1.87;Pneumatic control SL750;110;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 130x180;Mercor S.A.;Smoke vent mcr ULTRA THERM;13001800;0;250;560;154
E 130x190;Smoke vent;mcr ULTRA THERM;130x190 cm;1300;1900;1.59;1.68;1.98;Pneumatic control SL750;110;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 130x190;Mercor S.A.;Smoke vent mcr ULTRA THERM;13001900;0;250;560;154
E 130x200;Smoke vent;mcr ULTRA THERM;130x200 cm;1300;2000;1.66;1.77;2.08;Pneumatic control SL750;115;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 130x200;Mercor S.A.;Smoke vent mcr ULTRA THERM;13002000;0;250;560;354
E 130x210;Smoke vent;mcr ULTRA THERM;130x210 cm;1300;2100;1.73;1.86;2.18;Pneumatic control SL750;115;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 130x210;Mercor S.A.;Smoke vent mcr ULTRA THERM;13002100;0;250;560;354
E 130x220;Smoke vent;mcr ULTRA THERM;130x220 cm;1300;2200;1.81;1.94;2.29;Pneumatic control SL750;120;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 130x220;Mercor S.A.;Smoke vent mcr ULTRA THERM;13002200;0;250;560;354
E 130x230;Smoke vent;mcr ULTRA THERM;130x230 cm;1300;2300;1.88;2.03;2.39;Pneumatic control SL750;120;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 130x230;Mercor S.A.;Smoke vent mcr ULTRA THERM;13002300;0;250;560;354
E 130x240;Smoke vent;mcr ULTRA THERM;130x240 cm;1300;2400;1.95;2.12;2.5;Pneumatic control SL750;125;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 130x240;Mercor S.A.;Smoke vent mcr ULTRA THERM;13002400;0;250;560;354
E 130x250;Smoke vent;mcr ULTRA THERM;130x250 cm;1300;2500;2.01;2.21;2.6;Pneumatic control SL750;130;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 130x250;Mercor S.A.;Smoke vent mcr ULTRA THERM;13002500;0;250;560;354
C 140;Smoke vent;mcr ULTRA THERM;140x140 cm;1400;1400;1.28;1.35;1.57;Pneumatic control SL750;105;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM C 140;Mercor S.A.;Smoke vent mcr ULTRA THERM;14001400;0;175;284;214
E 140x150;Smoke vent;mcr ULTRA THERM;140x150 cm;1400;1500;1.36;1.45;1.68;Pneumatic control SL750;105;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 140x150;Mercor S.A.;Smoke vent mcr ULTRA THERM;14001500;0;175;465;214
E 140x160;Smoke vent;mcr ULTRA THERM;140x160 cm;1400;1600;1.44;1.54;1.8;Pneumatic control SL750;110;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 140x160;Mercor S.A.;Smoke vent mcr ULTRA THERM;14001600;0;175;465;194
E 140x170;Smoke vent;mcr ULTRA THERM;140x170 cm;1400;1700;1.52;1.63;1.91;Pneumatic control SL750;110;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 140x170;Mercor S.A.;Smoke vent mcr ULTRA THERM;14001700;0;175;465;174
E 140x180;Smoke vent;mcr ULTRA THERM;140x180 cm;1400;1800;1.6;1.71;2.02;Pneumatic control SL750;115;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 140x180;Mercor S.A.;Smoke vent mcr ULTRA THERM;14001800;0;175;465;174
E 140x190;Smoke vent;mcr ULTRA THERM;140x190 cm;1400;1900;1.68;1.82;2.14;Pneumatic control SL750;120;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 140x190;Mercor S.A.;Smoke vent mcr ULTRA THERM;14001900;0;175;465;174
E 140x200;Smoke vent;mcr ULTRA THERM;140x200 cm;1400;2000;1.76;1.9;2.24;Pneumatic control SL750;120;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 140x200;Mercor S.A.;Smoke vent mcr ULTRA THERM;14002000;0;175;465;154
E 140x210;Smoke vent;mcr ULTRA THERM;140x210 cm;1400;2100;1.84;2;2.37;Pneumatic control SL750;125;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 140x210;Mercor S.A.;Smoke vent mcr ULTRA THERM;14002100;0;175;465;154
E 140x220;Smoke vent;mcr ULTRA THERM;140x220 cm;1400;2200;1.92;2.09;2.46;Pneumatic control SL750;125;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 140x220;Mercor S.A.;Smoke vent mcr ULTRA THERM;14002200;0;175;465;394
E 140x230;Smoke vent;mcr ULTRA THERM;140x230 cm;1400;2300;1.99;2.19;2.58;Pneumatic control SL750;130;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 140x230;Mercor S.A.;Smoke vent mcr ULTRA THERM;14002300;0;175;465;394
E 140x240;Smoke vent;mcr ULTRA THERM;140x240 cm;1400;2400;2.07;2.28;2.69;Pneumatic control SL750;130;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 140x240;Mercor S.A.;Smoke vent mcr ULTRA THERM;14002400;0;250;560;394
E 140x250;Smoke vent;mcr ULTRA THERM;140x250 cm;1400;2500;2.14;2.38;2.8;Pneumatic control SL750;135;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 140x250;Mercor S.A.;Smoke vent mcr ULTRA THERM;14002500;0;250;560;394
C 150;Smoke vent;mcr ULTRA THERM;150x150 cm;1500;1500;1.43;1.55;1.8;Pneumatic control SL750;110;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM C 150;Mercor S.A.;Smoke vent mcr ULTRA THERM;15001500;0;175;465;214
E 150x160;Smoke vent;mcr ULTRA THERM;150x160 cm;1500;1600;1.52;1.63;1.92;Pneumatic control SL750;115;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 150x160;Mercor S.A.;Smoke vent mcr ULTRA THERM;15001600;0;175;465;214
E 150x170;Smoke vent;mcr ULTRA THERM;150x170 cm;1500;1700;1.61;1.74;2.05;Pneumatic control SL750;120;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 150x170;Mercor S.A.;Smoke vent mcr ULTRA THERM;15001700;0;175;465;194
E 150x180;Smoke vent;mcr ULTRA THERM;150x180 cm;1500;1800;1.69;1.84;2.16;Pneumatic control SL750;120;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 150x180;Mercor S.A.;Smoke vent mcr ULTRA THERM;15001800;0;175;465;194
E 150x190;Smoke vent;mcr ULTRA THERM;150x190 cm;1500;1900;1.78;1.94;2.29;Pneumatic control SL750;125;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 150x190;Mercor S.A.;Smoke vent mcr ULTRA THERM;15001900;0;175;465;174
E 150x200;Smoke vent;mcr ULTRA THERM;150x200 cm;1500;2000;1.86;2.04;2.43;Pneumatic control SL750;125;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 150x200;Mercor S.A.;Smoke vent mcr ULTRA THERM;15002000;0;175;465;174
E 150x210;Smoke vent;mcr ULTRA THERM;150x210 cm;1500;2100;1.95;2.14;2.55;Pneumatic control SL750;130;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 150x210;Mercor S.A.;Smoke vent mcr ULTRA THERM;15002100;0;175;465;174
E 150x220;Smoke vent;mcr ULTRA THERM;150x220 cm;1500;2200;2.03;2.24;2.66;Pneumatic control SL750;135;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 150x220;Mercor S.A.;Smoke vent mcr ULTRA THERM;15002200;0;175;465;154
E 150x230;Smoke vent;mcr ULTRA THERM;150x230 cm;1500;2300;2.11;2.34;2.76;Pneumatic control SL750;135;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 150x230;Mercor S.A.;Smoke vent mcr ULTRA THERM;15002300;0;175;465;434
E 150x240;Smoke vent;mcr ULTRA THERM;150x240 cm;1500;2400;2.19;2.45;2.88;Pneumatic control SL750;140;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 150x240;Mercor S.A.;Smoke vent mcr ULTRA THERM;15002400;0;250;560;434
C 160;Smoke vent;mcr ULTRA THERM;160x160 cm;1600;1600;1.6;1.74;2.05;Pneumatic control SL750;120;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM C 160;Mercor S.A.;Smoke vent mcr ULTRA THERM;16001600;0;195;510;234
E 160x170;Smoke vent;mcr ULTRA THERM;160x170 cm;1600;1700;1.69;1.85;2.19;Pneumatic control SL750;120;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 160x170;Mercor S.A.;Smoke vent mcr ULTRA THERM;16001700;0;195;510;214
E 160x180;Smoke vent;mcr ULTRA THERM;160x180 cm;1600;1800;1.78;1.96;2.33;Pneumatic control SL750;125;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 160x180;Mercor S.A.;Smoke vent mcr ULTRA THERM;16001800;0;195;510;214
E 160x190;Smoke vent;mcr ULTRA THERM;160x190 cm;1600;1900;1.87;2.07;2.46;Pneumatic control SL750;130;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 160x190;Mercor S.A.;Smoke vent mcr ULTRA THERM;16001900;0;195;510;194
E 160x200;Smoke vent;mcr ULTRA THERM;160x200 cm;1600;2000;1.96;2.18;2.59;Pneumatic control SL750;130;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 160x200;Mercor S.A.;Smoke vent mcr ULTRA THERM;16002000;0;195;510;194
E 160x210;Smoke vent;mcr ULTRA THERM;160x210 cm;1600;2100;2.05;2.28;2.71;Pneumatic control SL750;135;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 160x210;Mercor S.A.;Smoke vent mcr ULTRA THERM;16002100;0;195;510;174
E 160x220;Smoke vent;mcr ULTRA THERM;160x220 cm;1600;2200;2.13;2.39;2.85;Pneumatic control SL750;135;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 160x220;Mercor S.A.;Smoke vent mcr ULTRA THERM;16002200;0;195;510;174
E 160x230;Smoke vent;mcr ULTRA THERM;160x230 cm;1600;2300;2.22;2.5;2.98;Pneumatic control SL750;140;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 160x230;Mercor S.A.;Smoke vent mcr ULTRA THERM;16002300;0;195;510;174
E 160x240;Smoke vent;mcr ULTRA THERM;160x240 cm;1600;2400;2.3;2.61;3.11;Pneumatic control SL750;145;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 160x240;Mercor S.A.;Smoke vent mcr ULTRA THERM;16002400;0;195;510;174
E 160x250;Smoke vent;mcr ULTRA THERM;160x250 cm;1600;2500;2.39;2.7;3.24;Pneumatic control SL750;145;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 160x250;Mercor S.A.;Smoke vent mcr ULTRA THERM;16002500;0;195;510;574
C 170;Smoke vent;mcr ULTRA THERM;170x170 cm;1700;1700;1.77;1.97;2.34;Pneumatic control SL750;125;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM C 170;Mercor S.A.;Smoke vent mcr ULTRA THERM;17001700;0;195;510;234
E 170x180;Smoke vent;mcr ULTRA THERM;170x180 cm;1700;1800;1.87;0;2.47;Pneumatic control SL750;130;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 170x180;Mercor S.A.;Smoke vent mcr ULTRA THERM;17001800;0;195;510;234
E 170x190;Smoke vent;mcr ULTRA THERM;170x190 cm;1700;1900;1.96;2.19;2.61;Pneumatic control SL750;135;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 170x190;Mercor S.A.;Smoke vent mcr ULTRA THERM;17001900;0;195;510;214
E 170x200;Smoke vent;mcr ULTRA THERM;170x200 cm;1700;2000;2.06;2.3;2.74;Pneumatic control SL750;135;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 170x200;Mercor S.A.;Smoke vent mcr ULTRA THERM;17002000;0;195;510;214
E 170x210;Smoke vent;mcr ULTRA THERM;170x210 cm;1700;2100;2.15;2.41;2.88;Pneumatic control SL750;140;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 170x210;Mercor S.A.;Smoke vent mcr ULTRA THERM;17002100;0;250;698;194
E 170x220;Smoke vent;mcr ULTRA THERM;170x220 cm;1700;2200;2.24;2.53;3.02;Pneumatic control SL750;145;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 170x220;Mercor S.A.;Smoke vent mcr ULTRA THERM;17002200;0;250;698;194
E 170x230;Smoke vent;mcr ULTRA THERM;170x230 cm;1700;2300;2.33;2.64;3.16;Pneumatic control SL750;145;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 170x230;Mercor S.A.;Smoke vent mcr ULTRA THERM;17002300;0;250;698;194
E 170x240;Smoke vent;mcr ULTRA THERM;170x240 cm;1700;2400;2.42;2.75;3.3;Pneumatic control SL750;150;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 170x240;Mercor S.A.;Smoke vent mcr ULTRA THERM;17002400;0;250;698;174
E 170x250;Smoke vent;mcr ULTRA THERM;170x250 cm;1700;2500;2.51;2.86;3.44;Pneumatic control SL750;150;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 170x250;Mercor S.A.;Smoke vent mcr ULTRA THERM;17002500;0;250;698;174
C 180;Smoke vent;mcr ULTRA THERM;180x180 cm;1800;1800;1.95;2.2;2.62;Pneumatic control SL750;135;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM C 180;Mercor S.A.;Smoke vent mcr ULTRA THERM;18001800;0;195;510;234
E 180x190;Smoke vent;mcr ULTRA THERM;180x190 cm;1800;1900;2.05;2.31;2.76;Pneumatic control SL750;135;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 180x190;Mercor S.A.;Smoke vent mcr ULTRA THERM;18001900;0;195;510;234
E 180x200;Smoke vent;mcr ULTRA THERM;180x200 cm;1800;2000;2.15;2.45;2.92;Pneumatic control SL750;140;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 180x200;Mercor S.A.;Smoke vent mcr ULTRA THERM;18002000;0;250;698;214
E 180x210;Smoke vent;mcr ULTRA THERM;180x210 cm;1800;2100;2.25;2.55;3.06;Pneumatic control SL750;145;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 180x210;Mercor S.A.;Smoke vent mcr ULTRA THERM;18002100;0;250;698;214
E 180x220;Smoke vent;mcr ULTRA THERM;180x220 cm;1800;2200;2.34;2.65;3.21;Pneumatic control SL750;145;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 180x220;Mercor S.A.;Smoke vent mcr ULTRA THERM;18002200;0;250;698;214
E 180x230;Smoke vent;mcr ULTRA THERM;180x230 cm;1800;2300;2.44;2.79;3.35;Pneumatic control SL750;150;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 180x230;Mercor S.A.;Smoke vent mcr ULTRA THERM;18002300;0;250;698;194
E 180x240;Smoke vent;mcr ULTRA THERM;180x240 cm;1800;2400;2.53;2.89;3.5;Pneumatic control SL750;155;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 180x240;Mercor S.A.;Smoke vent mcr ULTRA THERM;18002400;0;250;698;194
E 180x250;Smoke vent;mcr ULTRA THERM;180x250 cm;1800;2500;2.63;3.02;3.65;Pneumatic control SL750;155;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 180x250;Mercor S.A.;Smoke vent mcr ULTRA THERM;18002500;0;250;698;194
C 190;Smoke vent;mcr ULTRA THERM;190x190 cm;1900;1900;2.14;2.45;2.92;Pneumatic control SL750;145;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM C 190;Mercor S.A.;Smoke vent mcr ULTRA THERM;19001900;0;250;850;254
E 190x200;Smoke vent;mcr ULTRA THERM;190x200 cm;1900;2000;2.24;2.55;3.08;Pneumatic control SL550;145;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL550  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 190x200;Mercor S.A.;Smoke vent mcr ULTRA THERM;19002000;0;250;850;234
E 190x210;Smoke vent;mcr ULTRA THERM;190x210 cm;1900;2100;2.34;2.69;3.23;Pneumatic control SL550;150;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL550  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 190x210;Mercor S.A.;Smoke vent mcr ULTRA THERM;19002100;0;250;850;234
E 190x220;Smoke vent;mcr ULTRA THERM;190x220 cm;1900;2200;2.45;2.81;3.39;Pneumatic control SL550;155;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL550  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 190x220;Mercor S.A.;Smoke vent mcr ULTRA THERM;19002200;0;250;850;234
E 190x230;Smoke vent;mcr ULTRA THERM;190x230 cm;1900;2300;2.55;2.94;3.54;Pneumatic control SL550;155;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL550  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 190x230;Mercor S.A.;Smoke vent mcr ULTRA THERM;19002300;0;250;850;214
E 190x240;Smoke vent;mcr ULTRA THERM;190x240 cm;1900;2400;2.64;3.06;3.7;Pneumatic control SL550;160;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL550  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 190x240;Mercor S.A.;Smoke vent mcr ULTRA THERM;19002400;0;250;850;214
E 190x250;Smoke vent;mcr ULTRA THERM;190x250 cm;1900;2500;2.74;3.19;3.85;Pneumatic control SL750;160;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL750  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 190x250;Mercor S.A.;Smoke vent mcr ULTRA THERM;19002500;0;250;850;214
C 195;Smoke vent;mcr ULTRA THERM;195x195 cm;1950;1950;2.24;2.55;3.08;Pneumatic control SL550;145;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL550  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM C 195;Mercor S.A.;Smoke vent mcr ULTRA THERM;19501950;0;250;850;254
E 195x200;Smoke vent;mcr ULTRA THERM;195x200 cm;1950;2000;2.29;2.61;3.16;Pneumatic control SL550;150;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL550  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 195x200;Mercor S.A.;Smoke vent mcr ULTRA THERM;19502000;0;250;850;254
E 195x220;Smoke vent;mcr ULTRA THERM;195x220 cm;1950;2200;2.5;2.87;3.48;Pneumatic control SL550;155;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL550  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 195x220;Mercor S.A.;Smoke vent mcr ULTRA THERM;19502200;0;250;850;234
C 200;Smoke vent;mcr ULTRA THERM;200x200 cm;2000;2000;2.33;2.68;3.24;Pneumatic control SL550;150;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL550  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM C 200;Mercor S.A.;Smoke vent mcr ULTRA THERM;20002000;0;250;850;254
E 200x210;Smoke vent;mcr ULTRA THERM;200x210 cm;2000;2100;2.44;2.83;3.4;Pneumatic control SL550;155;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL550  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 200x210;Mercor S.A.;Smoke vent mcr ULTRA THERM;20002100;0;250;850;254
E 200x220;Smoke vent;mcr ULTRA THERM;200x220 cm;2000;2200;2.55;2.96;3.57;Pneumatic control SL550;155;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL550  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 200x220;Mercor S.A.;Smoke vent mcr ULTRA THERM;20002200;0;250;850;234
E 200x230;Smoke vent;mcr ULTRA THERM;200x230 cm;2000;2300;2.65;3.09;3.73;Pneumatic control SL550;160;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL550  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 200x230;Mercor S.A.;Smoke vent mcr ULTRA THERM;20002300;0;250;850;234
E 200x240;Smoke vent;mcr ULTRA THERM;200x240 cm;2000;2400;2.75;3.22;3.89;Pneumatic control SL550;165;Straight base, made of galv. steel sheet with PVC frame;Base has to be insulated with thermal insulation layer of 50 mm (ie mineral wool), recommended lambda min 0,039 W/m/K.;https://www.mercor.com.pl/en/products/natural-smoke-exhausting/smoke-exhaust-vents/mcr-ultratherm-smoke-vents/;Pneumatic control SL550  Glazing: multiwall polycarbonate panel;mcr ULTRA THERM E 200x240;Mercor S.A.;Smoke vent mcr ULTRA THERM;20002400;0;250;850;234
