# This is a Revit shared parameter file.
# Do not edit manually.
*META	VERSION	MINVERSION
META	2	1
*GROUP	ID	NAME
GROUP	1	mcr
*PARAM	GUID	NAME	DATATYPE	DATACATEGORY	GROUP	VISIBLE	DESCRIPTION	USERMODIFIABLE
PARAM	2c13fc02-45bd-4893-a441-a125e91b2a83	mcr_Electric control - parameters	TEXT		1	1		1
PARAM	b7375a14-b7cb-49ff-8cee-685d6fa825ed	mcr_Smode vent with roof access function	YESNO		1	1		1
PARAM	07188319-858e-444b-b86b-87d4c92be289	mcr_Nominal length	LENGTH		1	1		1
PARAM	ded0c623-0015-45cb-9c27-b79c753714c7	mcr_Wind deflector	YESNO		1	1		1
PARAM	4f7fcd2c-b443-487c-b055-5d408417124e	mcr_Nominal dimensions (roof opening dim.)	TEXT		1	1		1
PARAM	1cad6f33-8119-47b5-81b7-d282f052f518	mcr_Notes	TEXT		1	1		1
PARAM	491db246-acb9-48de-89f0-b396eaca8fb1	mcr_Nominal width	LENGTH		1	1		1
PARAM	a814634c-17ea-4582-83b6-a8a10cd36e7c	mcr_Active_area	AREA		1	1		1
PARAM	ff03a259-e113-42c0-b728-3ddf4577e361	mcr_Smoke vent with roof access function	YESNO		1	1		1
PARAM	4e9cfd59-1fa1-48f5-abfd-f729cfa2ef63	mcr_Base height	FAMILYTYPE	-2000151	1	1		1
PARAM	48c6ee5e-0e0c-407d-bd9b-13f18fab4cab	mcr_Pneumatic control - parameters	TEXT		1	1		1
PARAM	dcff2b76-a437-4910-ad13-58781366d90e	mcr_Active area with wind deflectors	AREA		1	1		1
PARAM	f3b9fc7b-ca1a-4563-b083-71d5a004c919	mcr_Base type	TEXT		1	1		1
PARAM	9185c682-42cd-418d-8f6f-765d988dd661	mcr_Group	TEXT		1	1		1
PARAM	9269c79c-bed0-404a-8efa-f1e87f88cffc	mcr_Power consumption (at 24 V)	ELECTRICAL_CURRENT		1	1		1
PARAM	85d9b6a8-5f00-4a07-9244-518186676a92	mcr_Family	TEXT		1	1		1
PARAM	a7cc79c4-f664-47d8-97ce-0b5a0ff7744a	mcr_Wind and inlet deflector	YESNO		1	1		1
PARAM	906025e6-a780-4eae-acb1-d928fc40625d	mcr_Code	TEXT		1	1		1
PARAM	ab7072e6-4844-4f57-8d20-44f6ed691ee2	mcr_Active area with wind deflectors and inlet deflector	AREA		1	1		1
PARAM	0965f5e7-acca-4c54-ac3a-33bec8f55c43	mcr_Active area	AREA		1	1		1
PARAM	8a92f4f2-ff63-468f-9c46-02f3a932f51b	mcr_Weight	MASS		1	1		1
